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Description
Integrated 4K UHD camera, beam forming microphone, and full-range speakers, TV-MU650X(s) is specially designed for small and medium conference rooms, and micro-collaboration spaces with 4 to 6 people, helping enterprises to explore the use potential of internal small and micro meeting spaces. On the one hand, meetings can be held more efficiently, and on the other hand, rental costs can be saved.

Feature
* Using 1/2.5-inch and 8.51 million-pixel high-quality UHD CMOS sensor, with 4K (3840x2160)@30fps UHD clear images, and backward compatible with 1080P, 720P and other resolutions.
* 121° wide field of view (110° horizontal field of view), 5x zoom, optical lens specially tailored for conference scenes, built-in motorized pan/tilt (pan and tilt ±15° range of motion), which is easier to shoot conference personnel clearly.
* Built-in beam forming microphone, pickup distance of 6 meters, the low distortion lateral beam forming algorithm can guide the microphone directly to the speaker, for better sound, and clearer communication.
* Built-in audio 3A algorithm (AEC/AGC/ANS), full-duplex dialogue, can meet the communication needs of different room structures, whether sitting at the conference table, standing, people can comfortably and clearly communicate.
* Built-in intelligent analysis algorithm, identify the position according to the sound, automatically select the participants, automatically track the speaker, and switch the speaker screen to ensure that speaker is always clearly on the screen.
* Flexibly provide various installation options such as table top, wall hanging, TV/display hanging, and so on, which is easier and faster to install and deploy in crowded conference rooms.

Specification
	Video resolution
	4K@30fps，1080P@30fps，720P@60/30fps, etc.

	Sensor
	1/2.5 inch, CMOS, effective pixels: 8.51 million

	Optical lens
	121°(DFOV), 110°(HFOV), 5x zoom, pan/tilt ±15°

	PTZ
	Mechanical PTZ (MPT) + Electronic PTZ (EPTZ)

	Digital noise reduction
	2D&3D digital noise reduction

	SNR
	≥55dB

	BLC
	Support

	Full-range speaker
	96 dB SPL at 0.5 m

	Microphone array
	Beam forming microphone with pickup distance of 6 meters

	Connection type
	USB 3.0, backward compatible with USB2.0

	Color space/compression
	MJPEG/YUY2

	USB audio
	32K sampling rate, support UAC1.0

	USB video communication protocol
	UVC 1.1

	UVC PTZ control
	Support

	USB interface
	1*USB3.0, Type C ; 1*USB2.0, Type A ;

	Wireless
	Bluetooth data communication (Bluetooth 5.0)

	Installation method
	Support desktop, wall-mounted, TV-mounted and other installation options

	Standard cable
	USB cable

	Security
	Anti-theft lock jack

	Power supply
	DC 12V, 2A (MAX)

	Operating temperature
	0℃~40℃

	Storage temperature
	-40℃~60℃

	Product size (L*W*H)
	600×115.5×134.9mm

	Net weight
	2.5kg

	Scanning
	Progressive scanning

	Minimum illumination
	≤0.5 Lux

	Shutter
	Auto, manual, shutter priority, etc.

	White balance
	Auto, manual

	Output
	IP+USB, supports IP protocol RTSP

	PoE power supply
	Supports PoE+ power supply, complies with IEEE802.3at



Model Configuration Explanation
* TV-MU650X – Standard Configuration
This is the standard version normally shown in the general product datasheet.
* TV-MU650X(s) – Special Factory Configuration
* This is the same TV-MU650X product family and the same basic equipment platform, but supplied from the factory with additional or enhanced technical characteristics available according to the customer's project requirements.
* The letters (s) only identify the specific factory configuration supplied under this model. The main product family remains the standard model
因产品不断升级改进，本图册所提供的产品图片及技术参数等仅供参考，请以产品实物为准
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